**2. List of related services, and Implementation schedule (none):**

**3. Summary of technical specifications**

 **Tricycles must conform to the following specification:**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Item** | **DESCRIPTION** |  **Technical specifications requested** | **UNITY** | **QUANTITY** |  **Technical specifications offered** |
| 1 | **Lot 1: MOTO TRICYCLE** |  **TRICYCLE MOTORCYCLE**:**Wagon**, minimum dimensions (L \* W \* H): 1.9m \* 1.2m \* 0.38m.**Engine**: Single cylinder.**Displacement**: 200cc to 220cc.**Empty weight**: 350kg to 400kg.**Maximum load**: 1.3 T to 1.6 T.**Max Speed**: Greater than 60km / h.**Transmission**: 5 speeds.**Steering system**: Handlebars.**Starting system**: Two systems (electric and by kick).Tank capacity: 15 to 20 L.**Frame**: Steel.Suspension: Leaf spring.**Consumption**: less than 4L / 100kmFuel.**Wheel size**: 5.00-12 or equivalent.**Spare wheels**: One spare wheel.Clutch: Manual.Battery: 12V. |  **U** | **1.800** |  |
| **2** | **LOT 2:****FLYING TRICYCLE WITHOUT CABIN** |  **Wagon**, minimum dimensions (L \* W \* H): 2.2m \* 1.2m \* 0.38m.Minimum distance from the **ground**: greater than 250mm.Engine power: between 20HP to 24 HP.D**isplacement**: 1000cc to 1200cc.**Fuel**: DieselEmpty weight: 1.1T to 1.2T.**Payload**: from 2.9T to 3.1T.Gross vehicle weight: 4.18T to 4.48T.**Max Speed**: Greater than 40km / h.**Steering system**: Steering wheel.**Maximum slope of ascent**: Greater than 13%.**Braking system**: Oil brake.**Cabin space**: 2 places.**Front wheel**: 6.00-14 or equivalent.**Rear wheel**: 6.00-14 or 7.5-16 or equivalent.Spare wheels: 1 Spare wheel.Battery: 12V. | **U** | **125** |  |
| **3** | **FLYWHEEL ISOTHERMAL TRICYCLE WITH CAB** |  **Car size** : minimum dimensions (**L \* W \* H**) : 5.1m \* 1.6m \* 1.6m.**Container size** : minimum dimensions (L \* W \* H) : 2.7m \* 1.6m \* 1.6m.Minimum distance from the **ground**: Greater than 210mm.**Engine power**: between 35HP to 40 HP.**Displacement**: 1600cc to 1900cc.Fuel: Diesel.**Empty weight**: 1.9T to 2.1T.**Payload**: from 3.9T to 4.1T.**Gross vehicle weight**: 5.8 T to 6.2T.**Max Speed**: Greater than 65km / h.**Steering system**: Steering wheel.**Maximum slope of ascent**: Greater than 13%.**Braking system**: Oil brake.**Cabin space**: 2 places.**Front wheel**: 6.00-14 or equivalent.**Rear wheel**: 6.00-14 or equivalent.**Spare wheels**: a Spare wheel.Battery: 12V. | **U** | **75** |  |

 **NOTE WELL**:

- The tenderer must mention the make, model, origin and manufacturer of the tricycles offered and communicate in his tender the catalogs of the tricycles offered.

-Guarantee for equipment against any manufacturing defect from the date of provisional acceptance, Duration: 12 months.